**Firmware Programming Notes for Auto-Ohm 10**

**Using Thumb-Drive**

Please use the following steps to program the Auto-Ohm 10

1. Copy the “aohm10.hex” file to the USB thumb drive.

2. Turn off Auto-Ohm power.

3. Insert thumb drive into the Auto-Ohm 10 USB memory port (on the Auto-Ohm 10 PCB).

4. Hold “Control Knob” on the Auto-Ohm 10 and turn on power.

5. Unit will reprogram itself.

6. Verify new firmware revision when the Auto-Ohm 10 restarts itself.